{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["SUBWOOFER_GENERAL_DATA","CEA2010_OUTPUT_RESULTS","SWEEP_OUTPUT_RESULTS","BASSAHOLIC_ROOM_SIZE","CEA2010_MAX_SWEEP_COMPARISON"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SUBWOOFER_GENERAL_DATA","index":0,"n_rows":66,"n_cols":11,"rows_kept":66,"cut":false,"hidden":false,"merged":[]}
["POWERED SUBWOOFER GENERAL INFORMATION INDEX"]
["Copyright © Audioholics.com / Josh Ricci 2016"]
[]
[null,"RETAIL","MANUFACTURER'S","DIMENSIONS","EXTERNAL VOLUME","WEIGHT","DRIVER","AMPLIFIER","SYSTEM","MULTIPLE","BUILT IN"]
["MANUFACTURER & MODEL","PRICE","WARRANTY","LxWxH (inches)","(cubic feet) / (liters)","(lbs) / (kilograms)","CONFIG","POWER RATING","TYPE","MODES?","PEQ?"]
["APERION: BRAVUS II 12D",899.0,"10 years / 2 electronics","15.5x15.5x17","2.36 / 67.3","62 / 28.1","1x12\"","650w","reflex (PR's)","NO","NO"]
["B&W: ASW-610XP",1199.0,"5 years / 2 electronics","14.8x12.8x12.8","1.4 / 39.6","34.4 / 15.6","1x10\"","500w","sealed","NO","YES"]
["BIC ACOUSTECH: PL-200",279.0,"8 years / 2 electronics","19.5x14.75x17.25","2.88 / 81.6","47 / 21.3","1x12\"","250w","bass reflex","NO","NO"]
["CADENCE CSX-15 MKII",499.0,"2 years","18x19x21.5","4.26 / 120","88 / 40","1x15\"","300w","bass reflex","NO","NO"]
["ELEMENTAL DESIGNS: A7S-450",849.0,"1 year","23.5x22.25x22.75","6.88 / 195","130 / 59","1x18\"","1300w","sealed","NO","NO"]
["EMOTIVA: X-REF12",599.0,"5 years","15.5x14.625x15.625","2.05 / 58.5","44 / 20","1X12\"","600w","sealed","NO","YES"]
["EPIK SUBWOOFERS: EMPIRE",799.0,"3 years","24x18x22","5.5 / 156","125 / 56.7","2x15\"","600w","sealed","NO","NO"]
["FUNK AUDIO FW18.0",3234.0,"3 years","20.5x22x22","5.7/ 164","95 / 43","1X18\"","2400W","sealed","NO","YES"]
["HSU: VTF-15H",879.0,"7 years / 2 electronics","25x18x26","6.8/191.7","120 / 54","1x15\"","350w","ported","YES","NO"]
["HSU: ULS-15 mk2",779.0,"7 years / 2 electronics","19.5x18x19","3.9 / 110","65 /29.4","1x15\"","600w","sealed","YES","NO"]
["JL AUDIO: E110",1500.0,"3 years","16.5x13.5x14.25","1.84 / 52",52.7,"1x10\"","1200w","sealed","NO","NO"]
["JL AUDIO: E112",1900.0,"3 years","18.4x15.5x16.25","2.68 / 75.8",73.5,"1x12\"","1500w","sealed","NO","NO"]
["KLIPSCH: SW-311",1599.0,"2 years","16.25x13x13.4375","1.64 / 46.4","37 / 16.8","1x10\"","500w","reflex (PR's)","NO","YES"]
["MARTIN LOGAN DYNAMO 1500X",1595.0,"3 years","18.3x16.75x17.6","3.125 / 90","52 / 23.6","1x15\"","650w","sealed","NO","NO"]
["OUTLAW AUDIO: LFM-1 EX",649.0,"3 years","24x17x22.75","5.31 / 150","80 / 36.3","1x12\"","350w","bass reflex","YES","NO"]
["PARADIGM SIGNATURE SUB 2",8999.0,"5 years / 3 electronics","22.375x23.75x24.5","7.5 / 214","230 / 104.3","6x10\"","4500w","sealed","NO","YES"]
["POWERSOUND: XV-15",799.0,"5 years","23.5x18.5x24.25","6.1 / 174","92 / 42","1x15\"","500w","bass reflex","NO","NO"]
["PREMIER ACOUSTICS: PA-150",349.0,"5 years / 2 electronics","19x18x21","4.2 / 119","69 / 31.3","1x15\"","250w","bass reflex","NO","NO"]
["RBH SOUND: SX-12",1099.0,"5 years / 1 electronics","21.125x17.7x19.625","4.25 / 120","53 / 24","1x12\"","350w","bass reflex","NO","NO"]
["RBH SOUND: SX-1212R",5300.0,"5 years / 1 electronics","17.75x38.5x21","8.3 / 237","130 / 59","2x12\"","2400w","bass reflex","NO","NO"]
["RYTHMIK AUDIO: FV15HP",1199.0,"5 years / 2 electronics","26x18x24","6.5 / 184","110 / 49.9","1x15\"","600w","bass reflex","YES","YES"]
["SVS: PB12-NSD",769.0,"5 years","22x17.3x20.9","4.6 / 131","66 / 30","1x12\"","400w","bass reflex","NO","NO"]
["SVS: PB13-ULTRA SLEDGE DSP",1999.0,"5 years","29.25x20.5x22.5","7.8 / 221","155 / 70.3","1x13.5\"","1000w","reflex / seal","YES","YES"]
["SVS PC2000",799.0,"5 years","16.6x16.6x34","4.3 / 121","50 / 22.7","1x12\"","500w","bass reflex","NO","NO"]
["SVS: SB12-NSD",649.0,"5 years","14.2x14.2x14.6","1.7 / 48.5","35 / 16","1x12\"","400w","sealed","NO","NO"]
["SVS: SB13-ULTRA",1599.0,"5 years","17.4x17.4x17.4","3.1 / 87","92 / 42","1x13.5\"","1000w","sealed","NO","YES"]
["VELODYNE: DD18+ ",4999.0,"2 years","25.6x20.67x22.72","6.9 / 197","142 / 64.4","1X18\"","1250w","sealed","NO","YES"]
["VELODYNE: EQ-MAX 15",879.0,"2 years","21x19x21.5","5 / 142","75 / 34","1x15\"","750w","bass reflex","NO","YES"]
["XTZ Sound 3X12",2499.0,"5 years / 2 electronics","21.9x21.1x44.5","11.9 / 337","170.3 / 77.3","3x12\"","1500w","reflex / seal","YES","NO"]
[]
["Tested by Gene DellaSala, Mark Sanfilipo & Paul Apollonio"]
[null,"RETAIL","MANUFACTURER'S","DIMENSIONS","EXTERNAL VOLUME","WEIGHT","DRIVER","AMPLIFIER","SYSTEM","MULTIPLE","BUILT IN"]
["MANUFACTURER & MODEL","PRICE","WARRANTY","LxWxH (inches)","(cubic feet) / (liters)","(lbs) / (kilograms)","CONFIG","POWER RATING","TYPE","MODES?","PEQ?"]
["Aperion Audio: Bravus 10D",799.0,"10 years /3 electronics","13.5x15x13.5","1.58/44.8","44 / 20","2x10\"","300w","sealed","YES","NO"]
["Axiom Audio: EP400v3",1145.0,"5 years","13.8x10.5x16.8","1.41/39.9","48 / 22","1x8\"","500w","sealed","YES","NO"]
["Axiom Audio: EP500v1",1270.0,"5 years","19.5x15x19.5","3.3/93.5","72.6 / 32.9","1 x 12\"","500w","ported","NO","NO"]
["Axiom Audio: EP600v1",1860.0,"5 years","45.5x 15x 17","6.7/190.1","103 / 46.9","1 x 12\"","600w","ported","NO","NO"]
["Emotiva: Xref-10",499.0,"5 years transferrable","13.6x12.6x13.6","1.35/38.2","33 / 15","1x10\"","300w","sealed","YES","NO"]
["Emotiva: Ultra 12",499.0,"5 years transferrable","13.6x12.6x13.6","1.35/38.2","38 / 17.2","1 x12\"","300w","sealed","NO","NO"]
["EMPtek ES1010i",499.0,"5 years/1 year electronics","13x19x27.5","3.9/111.3","45 / 20.4","2x10\"","250w","ported","NO","NO"]
["Funkywaves: FW 12.X",1750.0,"not specified","24x14.5x24","4.83/136.9","115 / 52.1","1x12\"","2000w","ported","NO","NO"]
["Lava: LSP12",338.0,"5 years","16.4x13.8x18.9","2.5 / 70.8","44.7 / 20.3","1 x 12\"","250w","ported","NO","NO"]
["JL Audio: f110",2100.0,"5 years","15.6x12.9 x17.3","2.01 / 57","67 / 30","1x10\"","900w","sealed","YES","YES"]
["RBH: S-10",499.0,"5 years/1 year electronics","13x15.5x16.5","1.92/54.5","33/15","1x10\"","150w","ported","NO","NO"]
["RBH: SX-10R",1299.0,"5 years/1 year electronics","15x15.25x18.5","2.45/69.4","45/20.4","1x10\"","350w","ported","NO","NO"]
["SVS: PB12-Plus DSP",1349.0,"3 years"," 25x 19x21","5.77/163.5","127 / 57.6","1 x 12.5\"","800w","ported","YES","YES"]
["Velodyne: DD-15",3999.0,"2 years","20x18x17.8","1.64 / 46.4","100 / 45","1x15\"","1250w","sealed","YES","YES"]
["Velodyne: DD-15+",4399.0,"2 years","20x18x22","4.6/129.8","120 / 54","1x15\"","1250w","sealed","YES","YES"]
["Velodyne: DD-18",4999.0,"2 years","21.3x23x19.3","5.5/155","120 / 54","1x18\"","1250w","sealed","YES","YES"]
{"$rows_empty":11}
["Last Update: 7/27/16"]

{"sheet":"CEA2010_OUTPUT_RESULTS","index":1,"n_rows":60,"n_cols":15,"rows_kept":60,"cut":false,"hidden":false,"merged":[]}
["CEA2010 MAX CLEAN RMS SUBWOOFER OUTPUT"]
["ALL DATA COLLECTED OUTDOORS / GROUND PLANE AND REFERENCED TO 2 METER RMS dB SPL VALUES"]
["Copyright © Audioholics.com / Josh Ricci 2016"]
[{"$nulls":7},"CEA2010",{"$nulls":5},"BANDWIDTH","FREQUENCY"]
[{"$nulls":7}," CENTER FREQUENCY",{"$nulls":5},"UNIFORMITY","RANGE"]
["MANUFACTURER & MODEL","10hz","12.5hz","16hz","20hz","25hz","31.5hz","40hz","50hz","63hz","80hz","100hz","125hz","20-80Hz","+/-3dB Window"]
["APERION: BRAVUS II 12D","/","/","/",87.0,100.2,105.3,109.8,112.6,112.2,110.7,109.8,109.3,"+/-12.8dB","40-125Hz"]
["B&W: ASW-610XP","/","/","/",85.1,90.0,96.1,101.5,105.9,108.9,108.1,106.2,104.9,"+/-11.9dB","50-125Hz"]
["BIC ACOUSTECH: PL-200","/","/","/",84.0,96.2,102.5,107.7,110.4,108.1,106.5,105.3,103.8,"+/-13.2dB","40-100Hz"]
["CADENCE CSX-15 MKII","/","/","/",83.8,89.7,93.3,98.6,109.3,115.5,120.2,119.3,116.8,"+/-18.2dB","63-125Hz"]
["ELEMENTAL DESIGNS: A7S-450","/",90.0,94.6,100.4,106.8,112.5,117.8,121.0,120.1,118.3,116.8,115.8,"+/-10.3dB","40-125Hz"]
["EMOTIVA: X-REF12","/","/","/",81.0,89.5,99.1,103.5,107.6,108.5,107.7,106.3,105.1,"+/-13.8dB","40-125Hz"]
["EPIK: EMPIRE","/",93.5,98.2,102.2,105.8,109.7,113.2,116.4,119.2,121.6,123.3,124.2,"+/-9.7dB","63-125Hz"]
["FUNK AUDIO: 18.0",91.9,95.5,99.2,103.6,108.8,114.9,119.9,121.4,121.9,121.7,121.6,121.6,"+/-9.2dB","40-125Hz"]
["HSU: VTF-15H:  SEALED, EQ1","/",88.2,92.4,96.9,102.6,109.4,111.5,112.3,113.3,114.2,114.7,115.4,"+/-8.7dB","31.5-125Hz"]
["HSU: VTF-15H:  1 PORT OPEN, EQ1","/",93.5,100.6,104.1,106.9,111.3,113.5,113.7,114.2,114.6,115.1,115.5,"+/-5.3dB","31.5-125Hz"]
["HSU: VTF-15H:  2 PORTS OPEN, EQ2","/","/",93.4,104.1,109.7,113.1,115.6,115.3,115.3,115.5,115.6,115.9,"+/-5.7dB","25-100Hz"]
["JL AUDIO: E110","/","/",89.1,93.3,98.6,104.2,108.7,112.2,113.4,113.0,111.8,111.2,"+/-10dB","40-125Hz"]
["JL AUDIO: E112","/",87.7,92.6,97.5,103.2,108.6,112.4,114.7,115.0,113.7,112.5,111.5,"+/-8.8dB","40-125Hz"]
["KLIPSCH: SW-311","/","/","/",84.2,97.9,102.6,105.3,108.6,111.4,112.2,111.5,110.6,"+/-14dB","50-125Hz"]
["MARTIN LOGAN: DYNAMO 1500X","/",89.9,92.6,97.4,101.4,105.3,110.0,114.1,115.3,114.4,113.2,112.1,"+/-9dB","40-125Hz"]
["OUTLAW AUDIO: LFM-1 EX: 18hz","/","/",97.5,102.1,104.7,107.2,110.5,112.4,113.3,113.3,112.9,112.8,"+/-5.6dB","31.5-125Hz"]
["OUTLAW AUDIO: LFM-1 EX: 25hz","/","/",86.9,101.0,107.3,110.7,112.3,113.7,113.8,113.7,113.1,112.8,"+/-6.4dB","31.5-125Hz"]
["PARADIGM SIGNATURE SUB 2",94.7,98.2,102.6,106.4,109.9,113.2,116.9,120.2,122.5,123.0,122.1,120.3,"+/-8.3dB","40-125Hz"]
["POWERSOUND: XV-15","/","/",98.1,102.7,106.2,109.6,113.7,116.6,114.7,112.5,110.8,109.3,"+/-7dB","40-100Hz"]
["PREMIER ACOUSTICS: PA-150","/","/","/",93.6,98.6,105.4,109.3,114.4,118.0,117.8,116.9,116.0,"+/-12.2dB","50-125Hz"]
["RBH SOUND: SX-12","/","/","/",87.7,98.0,108.0,111.1,113.7,112.7,112.1,111.7,111.6,"+/-13dB","31.5-125Hz"]
["RBH SOUND: SX-1212R","/",99.6,107.7,112.8,114.5,117.3,120.8,120.1,120.5,120.6,120.6,120.7,"+/-4dB","31.5-125Hz"]
["RYTHMIK AUDIO: FV15HP: 1 PORT MODE","/",98.5,104.0,108.3,111.7,115.3,117.8,118.0,117.9,117.8,117.6,117.2,"+/-4.9dB","31.5-125Hz"]
["RYTHMIK AUDIO: FV15HP: 2 PORTS MODE","/",89.8,102.1,108.1,113.1,117.0,119.5,119.1,118.8,118.4,118.2,118.1,"+/-5.7dB","31.5-125Hz"]
["SVS PB12-NSD","/","/",93.3,103.2,105.0,105.9,106.5,107.3,108.0,108.7,109.2,109.6,"+/-2.8dB","20-100Hz"]
["SVS SB12-NSD",null,81.1,87.7,91.9,96.3,101.0,104.6,106.4,107.6,108.2,108.5,108.5,"+/-8.2dB","40-125Hz"]
["SVS SB13-ULTRA",83.0,88.6,92.6,96.5,101.3,108.1,112.1,114.9,116.8,117.3,117.2,116.9,"+/-10.4dB","40-125Hz"]
["SVS: PB13-ULTRA: 15HZ MODE","/",89.3,105.1,109.2,111.1,113.6,116.4,116.7,115.9,114.8,113.8,113.4,"+/-3.8dB","25-125Hz"]
["SVS: PB13-ULTRA: 20HZ MODE","/","/",97.4,110.6,113.5,115.5,117.5,117.8,116.6,115.3,114.4,114.1,"+/-3.6dB","25-125Hz"]
["SVS: PB13-ULTRA: SEALED MODE","/",84.6,91.5,97.6,104.0,110.0,113.8,115.2,114.7,114.0,113.4,113.0,"+/-8.8dB","31.5-125Hz"]
["VELODYNE EQ-MAX 15","/","/","/",84.8,95.7,104.2,110.0,114.2,114.8,111.0,108.3,106.7,"+/-15dB","40-80Hz"]
["VELODYNE: DD18+ SERVO GAIN 1",84.6,89.2,98.8,103.4,108.3,113.0,115.8,116.8,115.3,113.5,112.1,110.5,"+/-6.7dB","31.5-125Hz"]
["VELODYNE: DD18+ SERVO GAIN 8",86.1,92.5,98.9,103.6,108.2,112.9,115.3,116.3,115.1,113.4,112.0,110.6,"+/-6.4dB","31.5-125Hz"]
["XTZ SOUND 3X12","/",97.0,106.1,111.5,115.5,118.8,121.8,122.4,122.4,122.6,123.1,123.4,"+/-5.6dB","31.5-125Hz"]
[]
["HIGHEST RECORDED VALUE"]
[]
["Tested by Paul Apollonio (Funk and SVS) and Joel Foust (RBH models)"]
[{"$nulls":7},"CEA2010",{"$nulls":5},"BANDWIDTH","FREQUENCY"]
[{"$nulls":7}," CENTER FREQUENCY",{"$nulls":5},"UNIFORMITY","RANGE"]
["MANUFACTURER & MODEL","10hz","12.5hz","16hz","20hz","25hz","31.5hz","40hz","50hz","63hz","80hz","100hz","125hz","20-60Hz","+/-3dB Window"]
["Funkywaves: FW 12.X","/","/","/",107.0,112.3,112.4,114.0,113.9,113.1,"/","/","/","+/-3.5dB","25-63Hz"]
["RBH: SX-10R","/","/","/","/",94.0,103.0,106.0,108.0,109.0,108.0,107.0,105.0,"+/-3.5dB","25-63Hz"]
["RBH: S-10","/","/","/","/","/",98.0,105.0,107.0,107.0,106.0,105.0,103.0,"+/-4.2dB","25-63Hz"]
["SVS: PB12-Plus DSP","/","/","/",107.0,109.5,111.5,114.3,115.3,115.3,"/","/","/","+/-4.2dB","25-63Hz"]
[]
["Tested by James Larson"]
[{"$nulls":7},"CEA2010",{"$nulls":5},"BANDWIDTH","FREQUENCY"]
[{"$nulls":7}," CENTER FREQUENCY",{"$nulls":5},"UNIFORMITY","RANGE"]
["MANUFACTURER & MODEL","10hz","12.5hz","16hz","20hz","25hz","31.5hz","40hz","50hz","63hz","80hz","100hz","125hz","20-80Hz","+/-3dB Window"]
["HSU ULS-15 MK2","/",90.7,95.0,99.4,104.7,110.4,115.3,117.8,118.2,118.1,117.7,117.7,"+/- 9.4dB","40-125Hz"]
["SVS PC2000","/","/",95.6,104.3,108.7,109.9,111.5,111.2,110.9,109.9,109.6,109.5,"+/-3.6dB","25-125Hz"]
[]
["Last Update: 7/27/16"]

{"sheet":"SWEEP_OUTPUT_RESULTS","index":2,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":false,"merged":[]}
["MAX RMS SUBWOOFER OUTPUT RECORDED VIA LONG DURATION SINE SWEEP"]
["ALL DATA COLLECTED OUTDOORS / GROUND PLANE AND REFERENCED TO 2 METER RMS dB SPL VALUES"]
["Copyright © Audioholics.com / Josh Ricci 2015"]
[{"$nulls":13},"BANDWIDTH","FREQUENCY"]
[{"$nulls":5},"  FREQUENCY",{"$nulls":7},"UNIFORMITY","RANGE"]
["MANUFACTURER & MODEL","10Hz","12.5Hz","16Hz","20Hz","25Hz","31.5Hz","40Hz","50Hz","63Hz","80Hz","100Hz","125Hz","20-80Hz","+/-3dB Window"]
["APERION: BRAVUS II 12D","/","/",83.2,90.1,97.4,102.1,103.7,104.6,101.6,101.9,102.0,101.8,"+/-7.3dB","31.5-125Hz"]
["B&W: ASW-610XP","/",80.8,86.1,88.8,92.8,96.7,100.7,104.1,105.7,104.0,103.6,101.3,"+/-8.4dB","38-125Hz"]
["BIC ACOUSTECH: PL-200","/","/",82.1,87.1,95.1,101.9,106.3,107.6,103.7,101.9,100.8,97.8,"+/-10.2dB","36-63Hz"]
["CADENCE CSX-15 MKII","/","/","/",88.5,92.4,96.5,101.8,106.8,113.3,119.0,116.0,113.4,"+/-15.3dB","63-125Hz"]
["ELEMENTAL DESIGNS: A7S-450",84.0,91.2,98.9,102.9,107.0,111.9,116.8,119.6,117.9,115.9,114.4,114.3,"+/-8.3dB","35-125Hz"]
["EMOTIVA: X-REF12","/","/","/",83.3,94.3,99.7,103.4,104.6,104.0,101.2,99.6,97.2,"+/-10.6dB","29-106Hz"]
["EPIK: EMPIRE",80.0,88.1,98.6,102.1,106.0,109.3,110.8,112.7,115.1,117.3,118.2,119.4,"+/-7.6dB","55-125Hz"]
["FUNK AUDIO 18.0",91.3,95.1,98.2,103.1,108.0,114.1,119.7,121.0,118.3,117.3,116.9,116.8,"+/-9.0dB","33.5-125Hz"]
["HSU: VTF-15H:  SEALED, EQ1",82.6,90.2,95.5,99.7,104.3,109.4,110.7,111.6,111.1,112.6,112.4,112.5,"+/-6.5dB","28.5-125Hz"]
["HSU: VTF-15H:  1 PORT OPEN, EQ1",84.4,93.1,100.7,104.4,107.1,111.0,112.9,113.3,112.4,113.5,113.1,113.1,"+/-4.6dB","26.5-125Hz"]
["HSU: VTF-15H:  2 PORTS OPEN, EQ2","/",83.0,95.0,102.0,109.4,112.8,115.5,115.0,113.2,114.1,113.6,113.2,"+/-6.8dB","26-125Hz"]
["JL AUDIO: E110",78.7,85.4,89.8,93.3,97.8,102.4,107.2,109.0,106.8,106.8,105.5,104.7,"+/-7.9dB","34-125Hz"]
["JL AUDIO: E112",81.9,88.9,94.1,97.5,101.9,106.8,108.8,108.0,106.6,107.2,106.9,105.4,"+/-5.7dB","27.5-125Hz"]
["KLIPSCH: SW-311","/","/","/",73.1,93.9,99.8,101.8,103.9,106.7,108.0,109.3,107.5,"+/-17.4dB","45-125Hz"]
["MARTIN LOGAN DYNAMO 1500X",81.9,87.6,92.6,96.3,100.7,105.4,109.8,114.5,113.1,111.9,110.8,110.3,"+/-9.1dB","36-125Hz"]
["OUTLAW AUDIO: LFM-1 EX: 18hz","/",85.4,97.0,101.8,103.0,104.7,107.7,109.8,111.3,110.5,110.0,108.3,"+/-4.7dB","35-125Hz"]
["OUTLAW AUDIO: LFM-1 EX: 25hz","/","/",89.0,99.5,106.5,109.2,110.6,111.8,112.1,111.1,111.0,109.4,"+/-6.3dB","25-125Hz"]
["PARADIGM SIGNATURE SUB 2",96.3,99.1,102.9,105.0,106.9,109.1,110.6,111.6,111.6,112.0,112.5,112.2,"+/-3.5dB","24-125Hz"]
["POWERSOUND: XV-15",82.3,92.2,98.5,101.4,103.7,106.4,109.2,111.5,111.2,110.2,107.8,106.8,"+/-5.1dB","31.5-125Hz"]
["PREMIER ACOUSTICS: PA-150","/",81.1,90.2,95.2,99.4,103.4,107.3,112.1,116.0,114.9,113.5,113.4,"+/-10.4dB","45-125Hz"]
["RBH SOUND: SX-12","/","/",81.6,91.1,98.7,105.8,109.2,110.8,109.8,108.6,108.4,107.1,"+/-9.8dB","31-125Hz"]
["RBH SOUND: SX-1212R",83.4,94.5,106.5,111.3,114.3,116.1,116.7,116.5,115.8,115.6,114.4,113.8,"+/-3dB","20-125Hz"]
["RYTHMIK AUDIO: FV15HP: 1 PORT MODE",89.0,97.8,104.0,107.6,110.8,112.4,112.6,113.4,113.0,111.0,107.3,105.3,"+/-2.9dB","20-100Hz"]
["RYTHMIK AUDIO: FV15HP: 2 PORTS MODE","/",85.5,100.9,106.9,112.1,114.7,114.8,115.9,115.6,113.8,110.3,108.7,"+/-4.5dB","22.5-105Hz"]
["SVS PB12-NSD","/","/",91.0,99.4,104.3,105.2,105.3,106.2,106.8,107.2,107.5,108.2,"+/-3.9dB","22-125Hz"]
["SVS SB12-NSD","/",79.4,87.3,92.0,96.3,100.0,103.5,105.4,107.1,107.6,107.6,107.3,"+/-7.8dB","37-125Hz"]
["SVS SB13-ULTRA",86.9,90.3,94.4,97.8,101.1,105.1,108.4,111.7,113.0,113.6,112.2,111.4,"+/-8dB","36.5-125Hz"]
["SVS: PB13-ULTRA: 15HZ MODE",79.8,92.5,104.8,107.9,109.4,112.2,114.8,113.3,112.9,111.0,110.1,108.6,"+/-3.4dB","23-125Hz"]
["SVS: PB13-ULTRA: 20HZ MODE","/",85.9,99.5,109.3,111.9,113.4,115.9,115.1,113.3,111.2,110.2,109.0,"+/-3.3dB","21-100Hz"]
["SVS: PB13-ULTRA: SEALED MODE",86.8,91.4,96.4,100.2,104.6,109.5,112.4,111.1,111.4,109.9,109.2,107.8,"+/-6.1dB","28-125Hz"]
["VELODYNE EQ-MAX 15","/","/",78.8,91.7,98.1,102.8,107.8,112.4,111.8,107.9,105.7,104.7,"+/-10.3dB","38-86Hz"]
["VELODYNE: DD18+ SERVO GAIN 1",88.3,94.6,99.5,103.3,107.8,113.0,116.1,113.6,110.8,108.7,107.4,104.8,"+/-6.4dB","28-63Hz"]
["VELODYNE: DD18+ SERVO GAIN 8",88.3,93.5,99.1,102.8,107.3,111.6,113.6,114.1,112.9,111.7,111.0,109.8,"+/-5.6dB","28-125Hz"]
["XTZ SOUND 3X12",70.7,92.0,101.5,107.6,112.7,116.3,118.5,118.6,118.2,118.3,118.0,118.2,"+/-6.4dB","28-63Hz"]
[]
["HIGHEST RECORDED VALUE"]
["All subwoofers tabulated above were tested by: Josh Ricci"]
["Results were generated using a sine-wave sweep of roughly 23 second long duration covering the range of 2-125Hz"]
[]
["MAX RMS SUBWOOFER OUTPUT RECORDED VIA LONG DURATION SINE SWEEP"]
["ALL DATA COLLECTED OUTDOORS / GROUND PLANE AND REFERENCED TO 2 METER RMS dB SPL VALUES"]
["Copyright © Audioholics.com 2015"]
[{"$nulls":13},"BANDWIDTH","FREQUENCY"]
[{"$nulls":8}," FREQUENCY",{"$nulls":4},"UNIFORMITY","RANGE"]
["MANUFACTURER & MODEL","10Hz","12.5Hz","16Hz","20Hz","25Hz","31.5Hz","40Hz","50Hz","63Hz","80Hz","100Hz","125Hz","20-80Hz","+/-3dB Window"]
["Aperion Audio: Bravus 10D","/","/","/",75.0,80.0,88.0,96.0,100.0,101.0,104.0,102.0,100.0,"+/-14.5dB","40-125Hz"]
["Axiom Audio: EP400v3","/","/","/",88.0,91.0,94.0,96.0,96.0,95.0,95.0,94.0,93.0,"+/-3.5dB","25-125Hz"]
["Axiom Audio: EP500v1","/","/","/",88.0,97.0,99.0,100.0,100.0,99.0,99.0,99.0,100.0,"+/-6dB","25-125Hz"]
["Axiom Audio: EP600v1","/","/","/",95.0,100.0,104.0,105.0,101.0,100.0,97.0,99.0,99.0,"+/-3dB","20-125Hz"]
["Emotiva: Xref-10","/","/","/",84.0,89.0,91.0,98.0,101.0,102.0,104.0,102.0,101.0,"+/-10dB","40-125Hz"]
["Emotiva: Ultra 12","/","/","/",84.0,92.0,96.0,102.0,106.0,107.0,104.0,104.0,102.0,"+/-11.5dB","40-125Hz"]
["EMPtek ES1010i","/","/","/",85.0,91.0,97.0,102.5,106.0,106.0,105.0,105.0,105.0,"+/-10.5dB","35Hz-125Hz"]
["JL Audio: f110","/","/","/",91.0,97.0,101.0,102.0,101.0,100.0,97.0,95.0,92.0,"+/-5.5dB","31.5-100Hz"]
["Lava: LSP12","/","/","/",65.0,78.0,88.0,101.0,105.0,110.0,105.0,100.0,95.0,"+/-20dB","31.5-125Hz"]
["RBH: S-10","/","/","/",80.5,89.0,95.6,101.49,104.7,104.8,103.4,102.2,100.36,"+/-11.5dB","35-125Hz"]
["RBH: SX-10R","/","/",76.1,86.1,95.6,102.2,104.7,105.5,106.4,105.2,103.9,102.3,"+/-9.6dB","29-125Hz"]
["Velodyne: DD-15","/","/","/",90.0,94.0,98.0,104.0,107.0,111.0,109.0,111.0,109.0,"+/-10.5dB","40-125Hz"]
["Velodyne: DD-15+","/","/","/",97.0,101.0,105.0,111.0,111.0,112.0,108.0,107.0,104.0,"+/-7.5dB","25-125Hz"]
["Velodyne: DD-18","/","/","/",94.0,99.0,105.0,111.0,114.0,114.0,114.0,113.0,111.0,"+/-10dB","25-125Hz"]
[]
[]
["HIGHEST RECORDED VALUE"]
["All subwoofers tabulated above were tested by: Gene DellaSala ,except the DD-18 and LSP12 which were tested by Mark Sanfilipo  and the RBH models tested by Joel Foust"]
["Subwoofers tested using a continuous reverse sine-wave sweep tend to track closely in SPL to CEA-2010 tests at low frequencies where the subwoofer is driver limited"]
["CEA-2010 tends to yield higher SPL #s at higher frequencies where the subwoofer is amplifier limited"]
[]
["MAX RMS SUBWOOFER OUTPUT RECORDED VIA LONG DURATION SINE SWEEP"]
["ALL DATA COLLECTED OUTDOORS / GROUND PLANE AND REFERENCED TO 2 METER RMS dB SPL VALUES"]
["Copyright © Audioholics.com 2016"]
[{"$nulls":13},"BANDWIDTH","FREQUENCY"]
[{"$nulls":8}," FREQUENCY",{"$nulls":4},"UNIFORMITY","RANGE"]
["MANUFACTURER & MODEL","10Hz","12.5Hz","16Hz","20Hz","25Hz","31.5Hz","40Hz","50Hz","63Hz","80Hz","100Hz","125Hz","20-80Hz","+/-3dB Window"]
["HSU ULS-15 MK2",74.4,86.3,96.0,100.3,104.7,109.3,113.8,116.2,116.1,115.2,114.6,114.6,"+/-8dB","40-125Hz"]
["SVS PC2000","/","/",95.4,104.1,107.3,109.6,109.9,109.0,108.9,108.7,108.1,107.1,"+/-2.9dB","20-125Hz"]
[]
["All subwoofers tabulated above were tested by: James Larson"]
["Results were generated using a sine-wave sweep of roughly 23 second long duration covering the range of 2-1250Hz"]
[]
["Last Update: 7/27/16"]

{"sheet":"BASSAHOLIC_ROOM_SIZE","index":3,"n_rows":65,"n_cols":5,"rows_kept":65,"cut":false,"hidden":false,"merged":[]}
["AUDIOHOLICS \"BASSAHOLIC\" SUBWOOFER RATINGS"]
["MAXIMUM SUGGESTED ROOM SIZE TO ENSURE ADEQUATE OUTPUT HEADROOM"]
["Copyright © Audioholics.com / Josh Ricci 2016"]
[]
[null,"MINIMUM PASSING CRITERIA BASED ON CEA2010 2 METER"]
[null,"GROUNDPLANE PEAK OUTPUT CONVERTED TO 4 METER 1/8TH SPACE"]
["                                                          31.5-63Hz SPL","<109db",">109db","115db","123db"]
[]
["                                                                 25Hz SPL","<103db",">103db","109db","117db"]
["                                                              ROOM SIZE","SMALL","MEDIUM","LARGE","EXTREME"]
["MANUFACTURER & MODEL","<1500cu ft","1500-3000cu ft","3000-5000cu ft",">5000cu ft"]
["APERION: BRAVUS II 12D",null,null,"CERTIFIED"]
["B&W: ASW-610XP","CERTIFIED"]
["BIC ACOUSTECH: PL-200",null,"CERTIFIED"]
["CADENCE CSX-15 MKII","CERTIFIED"]
["ELEMENTAL DESIGNS: A7S-450",null,null,"CERTIFIED"]
["EMOTIVA: X-REF12","CERTIFIED"]
["EPIK: EMPIRE",null,null,"CERTIFIED"]
["FUNK AUDIO: 18.0",null,null,null,"CERTIFIED"]
["HSU: VTF-15H SEALED, EQ1",null,null,"CERTIFIED"]
["HSU: VTF-15H 1 PORTS, EQ1",null,null,"CERTIFIED"]
["HSU: VTF-15H 2 PORTS, EQ2",null,null,null,"CERTIFIED"]
["JL AUDIO: E110",null,"CERTIFIED"]
["JL AUDIO: E112",null,null,"CERTIFIED"]
["KLIPSCH: SW-311",null,"CERTIFIED"]
["MARTIN LOGAN: DYNAMO 1500X",null,null,"CERTIFIED"]
["OUTLAW AUDIO: LFM-1 EX: 18hz",null,null,"CERTIFIED"]
["OUTLAW AUDIO: LFM-1 EX: 25hz",null,null,"CERTIFIED"]
["PARADIGM SIGNATURE SUB 2",null,null,null,"CERTIFIED"]
["POWERSOUND: XV-15",null,null,"CERTIFIED"]
["PREMIER ACOUSTICS: PA-150",null,"CERTIFIED"]
["RBH SOUND: SX-12",null,null,"CERTIFIED"]
["RBH SOUND: SX-1212R",null,null,null,"CERTIFIED"]
["RYTHMIK AUDIO: FV15HP: 1 PORT MODE",null,null,null,"CERTIFIED"]
["RYTHMIK AUDIO: FV15HP: 2 PORTS MODE",null,null,null,"CERTIFIED"]
["SVS PB12-NSD",null,null,"CERTIFIED"]
["SVS: PB13-ULTRA: 15HZ MODE",null,null,null,"CERTIFIED"]
["SVS: PB13-ULTRA: 20HZ MODE",null,null,null,"CERTIFIED"]
["SVS: PB13-ULTRA: SEALED MODE",null,null,"CERTIFIED"]
["SVS SB13-ULTRA",null,null,"CERTIFIED"]
["SVS SB12-NSD",null,"CERTIFIED"]
["VELODYNE EQ-MAX 15",null,"CERTIFIED"]
["VELODYNE: DD18+",null,null,null,"CERTIFIED"]
["XTZ SOUND 3X12",null,null,null,"CERTIFIED"]
[]
["Aperion Audio: Bravus 10D","CERTIFIED"]
["Axiom Audio: EP400v3","CERTIFIED"]
["Axiom Audio: EP500v1",null,"CERTIFIED"]
["Axiom Audio: EP600v1",null,"CERTIFIED"]
["Emotiva: Xref-10","CERTIFIED"]
["Emotiva: Ultra 12","CERTIFIED"]
["EMPtek ES1010i"]
["Funkywaves: FW 12.X",null,null,"CERTIFIED"]
["HSU ULS-15 mk2",null,null,"CERTIFIED"]
["JL Audio: f110",null,"CERTIFIED"]
["Lava: LSP12","CERTIFIED"]
["RBH S-10","CERTIFIED"]
["RBH SX-10/R",null,"CERTIFIED"]
["SVS: PB12-Plus DSP",null,null,"CERTIFIED"]
["SVS PC2000",null,null,"CERTIFIED"]
["Velodyne: DD-15",null,"CERTIFIED"]
["Velodyne: DD-15+",null,null,"CERTIFIED"]
["Velodyne: DD-18",null,null,"CERTIFIED"]
[]
["Last Update: 7/27/16"]

{"sheet":"CEA2010_MAX_SWEEP_COMPARISON","index":4,"n_rows":133,"n_cols":13,"rows_kept":133,"cut":false,"hidden":false,"merged":[[55,0,55,12],[65,0,65,12]]}
["CEA2010 VERSUS MAX SWEEP LEVEL COMPARISON"]
["VALUES ARE THE AMOUNT THAT CEA2010 PASSING RESULTS RECORDED COMPARED TO DURING THE MAXIMUM LEVEL LONG TERM SWEEP"]
["POSITIVE VALUES INDICATE HIGHER OUTPUT WITH CEA2010 / NEGATIVE VALUES INDICATE LESS OUTPUT RECORDED VIA CEA2010"]
["Copyright© Audioholics.com / Josh Ricci 2016"]
[{"$nulls":7}," CENTER FREQUENCY"]
["MANUFACTURER & MODEL","10hz","12.5hz","16hz","20hz","25hz","31.5hz","40hz","50hz","63hz","80hz","100hz","125hz"]
["APERION: BRAVUS II 12D","/","/","/",-3.1,2.8,3.2,6.1,8.0,10.6,8.8,7.8,7.5]
["BIC ACOUSTECH: PL-200","/","/","/",-3.1,1.1,0.6,1.4,2.8,4.4,4.6,4.5,6.0]
["B&W: ASW-610XP","/","/","/",-3.7,-2.8,-0.6,0.8,1.8,3.2,4.1,2.6,3.6]
["BIC ACOUSTECH: PL-200","/","/","/",-3.1,1.1,0.6,1.4,2.8,4.4,4.6,4.5,6.0]
["CADENCE CSX-15 MKII","/","/","/",-4.7,-2.7,-3.2,-3.2,2.5,2.2,1.2,3.3,3.4]
["ELEMENTAL DESIGNS: A7S-450","/",-1.2,-4.3,-2.5,-0.2,0.6,1.0,1.4,2.2,2.4,2.4,1.5]
["EMOTIVA: X-REF12","/","/","/",-2.3,-4.8,-0.6,0.1,3.0,4.5,6.5,6.7,7.9]
["EPIK: EMPIRE",-1.5,5.4,-0.3,0.1,-0.2,0.4,2.4,3.7,4.1,4.3,5.1,4.8]
["FUNK AUDIO: 18.0",0.5,0.4,1.0,0.5,0.8,0.8,0.2,0.4,3.6,4.4,4.7,4.8]
["HSU: VTF-15H SEALED, EQ1","/",-2.0,-3.1,-2.8,-1.7,0.0,0.8,0.7,2.2,1.6,2.3,2.9]
["HSU: VTF-15H 1 PORTS, EQ1","/",0.4,-0.1,-0.3,-0.2,0.3,0.6,0.4,1.8,1.1,2.0,2.4]
["HSU: VTF-15H 2 PORTS, EQ2","/","/",-1.6,2.1,0.3,0.3,0.1,0.3,2.1,1.4,2.0,2.7]
["JL AUDIO: E110","/","/",-0.7,0.0,0.8,1.8,1.5,3.2,6.4,6.2,6.3,6.5]
["JL AUDIO: E112","/",-1.2,-1.5,0.0,1.3,1.8,3.6,6.7,8.4,6.5,5.6,6.1]
["KLIPSCH: SW-311","/","/","/",11.1,4.0,2.8,3.5,4.7,4.7,4.2,2.2,3.1]
["MARTIN LOGAN: DYNAMO 1500X","/",2.3,-0.4,0.7,0.4,-0.2,0.2,-0.4,2.2,2.5,2.4,1.8]
["OUTLAW AUDIO: LFM-1 EX: 18hz","/","/",0.5,0.3,1.7,2.5,2.8,2.6,2.0,2.8,2.9,4.5]
["OUTLAW AUDIO: LFM-1 EX: 25hz","/","/",-2.1,1.5,0.8,1.5,1.7,1.9,1.7,2.6,2.1,3.4]
["PARADIGM SIGNATURE SUB 2",-1.6,-0.9,-0.3,1.4,3.0,4.1,6.3,8.6,10.9,11.0,9.6,8.1]
["POWERSOUND: XV-15","/","/",-0.4,1.3,2.5,3.2,4.5,5.1,3.5,2.3,3.0,2.5]
["PREMIER ACOUSTICS: PA-150","/","/","/",-1.6,-0.8,2.0,2.0,2.3,2.0,2.9,3.4,2.6]
["RBH SOUND: SX-12","/","/","/",-3.4,-0.7,2.2,1.9,2.9,3.9,3.5,3.3,4.5]
["RYTHMIK AUDIO: FV15HP: 1 PORT MODE","/",0.7,0.0,0.7,0.9,2.9,5.2,4.6,4.9,6.9,10.3,11.9]
["RYTHMIK AUDIO: FV15HP: 2 PORTS MODE","/",4.3,1.2,1.2,1.0,2.3,4.7,3.2,3.2,4.6,7.9,9.4]
["SVS PB12-NSD","/","/",2.3,3.8,0.7,0.7,1.2,1.1,1.2,1.5,1.7,1.4]
["SVS: PB13-ULTRA: 15HZ MODE","/",-3.2,0.3,1.3,1.7,1.4,1.6,3.4,3.0,3.8,3.7,4.8]
["SVS: PB13-ULTRA: 20HZ MODE","/","/",-2.1,1.3,1.6,2.1,1.6,2.7,3.3,4.1,4.2,5.1]
["SVS: PB13-ULTRA: SEALED MODE","/",-6.8,-4.9,-2.6,-0.6,0.5,1.4,4.1,3.3,4.1,4.2,5.2]
["SVS SB12-NSD","/",1.7,0.4,-0.1,0.0,1.0,1.1,1.0,0.5,0.6,0.9,1.2]
["VELODYNE EQ-MAX 15","/","/","/",-6.9,-2.4,1.4,2.2,1.8,3.0,3.1,2.6,2.0]
["VELODYNE: DD18+ SERVO GAIN 1",-4.6,-5.4,-0.7,0.1,0.5,0.0,-0.3,3.2,4.5,4.8,4.7,5.7]
["VELODYNE: DD18+ SERVO GAIN 8",-3.0,-1.0,-0.2,0.8,0.9,1.3,1.7,2.2,2.2,1.7,1.0,0.8]
["XTZ SOUND 3X12","/",5.0,4.6,3.9,2.8,2.5,3.3,3.8,4.2,4.3,5.0,5.1]
["TOTAL RANGE OF VARIATION ALL UNITS / SPL dB",5.1,12.2,9.5,18.0,8.8,7.3,9.5,9.0,10.4,10.4,9.4,11.1]
["AVERAGE RANGE OF VARIATION ALL UNITS / SPL dB",-2.04,-0.09375,-0.539130434782609,-0.245454545454546,0.412121212121212,1.21818181818182,1.92121212121212,2.92424242424242,3.76666666666667,3.90909090909091,4.08787878787879,4.52121212121212]
["TOTAL AVERAGE VARIATION ALL UNITS / ALL FREQS",2.10821114369501]
["LEAST GAIN OR MOST LOSS"]
["MOST GAIN OR LEAST LOSS"]
[]
[]
[]
["CEA2010 VERSUS MAX SWEEP LEVEL COMPARISON"]
["VALUES ARE THE AMOUNT THAT CEA2010 PASSING RESULTS RECORDED COMPARED TO DURING THE MAXIMUM LEVEL LONG TERM SWEEP"]
["POSITIVE VALUES INDICATE HIGHER OUTPUT WITH CEA2010 / NEGATIVE VALUES INDICATE LESS OUTPUT RECORDED VIA CEA2010"]
["Copyright© Audioholics.com / Josh Ricci 2016"]
[{"$nulls":7}," CENTER FREQUENCY"]
["MANUFACTURER & MODEL","10hz","12.5hz","16hz","20hz","25hz","31.5hz","40hz","50hz","63hz","80hz","100hz","125hz"]
["RBH: S-10","/","/","/","/",-1.6,0.8,1.3,2.5,2.6,2.8,3.1,2.7]
["RBH: SX-10R","/","/","/","/","/",-2.4,3.5,2.3,2.2,2.6,2.8,2.6]
["Tested by: Joel Foust"]
[]
["CEA2010 VERSUS MAX SWEEP LEVEL COMPARISON"]
["VALUES ARE THE AMOUNT THAT CEA2010 PASSING RESULTS RECORDED COMPARED TO DURING THE MAXIMUM LEVEL LONG TERM SWEEP"]
["POSITIVE VALUES INDICATE HIGHER OUTPUT WITH CEA2010 / NEGATIVE VALUES INDICATE LESS OUTPUT RECORDED VIA CEA2010"]
["Copyright© Audioholics.com / Josh Ricci 2016"]
[{"$nulls":7}," CENTER FREQUENCY"]
["MANUFACTURER & MODEL","10hz","12.5hz","16hz","20hz","25hz","31.5hz","40hz","50hz","63hz","80hz","100hz","125hz"]
["HSU ULS-15 MK2","/",4.4,-1.0,-0.9,0.0,1.1,1.5,1.6,2.1,2.9,3.1,3.1]
["SVS PC2000","/","/",0.2,0.3,1.4,0.3,1.9,2.2,2.0,1.2,1.5,2.4]
["Tested by: James Larson"]
[]
["Last Update: 7/27/16"]
{"$rows_empty":51}
["FREQUENCY / DIY or passive stuff / FOR FURTHER REF","21SW152 P","DTS10","DTS LMSR","GJALLER","LMSR PR","LMSR SEA","AVERAGE","VARIATION"]
[10.0,null,-5.0,-7.0,-7.0,null,-6.1,-6.275,2.0]
[12.5,null,0.3,0.3,0.3,-0.6,-4.3,-0.8,4.6]
[16.0,2.3,2.2,0.7,3.6,-1.1,-3.1,0.766666666666667,6.7]
[20.0,2.0,0.4,1.3,1.4,-0.6,-1.4,0.516666666666667,3.4]
[25.0,2.8,1.0,2.1,0.8,0.4,-0.5,1.1,3.3]
[31.5,-0.4,0.3,5.1,3.0,0.0,-0.4,1.26666666666667,5.5]
[40.0,-1.0,3.8,1.7,5.0,1.7,1.8,2.16666666666667,6.0]
[50.0,1.4,4.3,4.0,4.3,4.1,4.6,3.78333333333333,3.2]
[63.0,3.7,7.5,8.6,4.0,5.3,6.6,5.95,4.9]
[80.0,4.3,7.1,5.9,5.7,7.2,7.1,6.21666666666667,2.9]
[100.0,4.7,4.2,5.4,5.0,6.8,8.5,5.76666666666667,4.3]
[125.0,4.5,13.9,9.6,1.0,7.4,7.9,7.38333333333333,12.9]
["TOTAL AVERAGE VARIATION SPL dB",2.88109318996416]